**SPECIFICATIONS FOR SPECTROPHOTOMETER**

MONOCHROMATOR:1200 GLOVES/MM DIFFRACTION GRATING MONOCHROMATOR.

OPTICAL SYSTEM:

DOUBLE BE LIGHT BAM LIGHT PATH THROUGH SAMPLE:10 MM,

SPECTRA BANDWIDTH: 0.5,1,2,4NM,

WAVELENGTH RANGE: 190-1100NM (0.1NM INCREMENT WAVELENGTH ACCURACY