**SPECIFICATIONS FOR ALGAE FLOC**

|  |  |  |
| --- | --- | --- |
| **No** | **ITEM** | **SPECIFICATIONS** |
| 1 | ALGAE FLOC 19s-Flocculants | Typical properties: Liquid polymer blend |
| Appearance and odour: Clear, orange/yellow liquid |
| Specific gravity@25ºc:1.175-1.210 |
| pH(neat):4.0ph units max |
| Solubility: Soluble in water |
| Viscosity@ 25ºc:30-100cps |
| Usage:Flocculant for drinking water |
| Certification:NSF to ANSI/NSF Standard 60 |
| Packaging: The product shall be presented in 250kg plastic drums clearly labelled with the following information; Net content, Batch/Lot Number, Name of Manufacturer and Address, Manufacturer and Expiry Dates, Manufacturer’s Quality Assurance Product Test Report |